HP P22va G4 FHD Monitor Specifications Table:
•	Display type VA
•	Brightness 250 nits
•	Contrast ratio 3000:1
•	Response Ratio 7ms GtG (with overdrive)
•	Product colour Black
•	Aspect ratio 16:9
•	Native resolution FHD (1920 x 1080)
•	Resolutions supported
•	1024 x 768; 1280 x 1024; 1280 x 720; 1280 x 800; 1440 x 900; 1600 x 900; 1680 x 1050; 1920 x 1080; 640 x 480; 720 x 400; 800 x
•	600
•	Display features Anti-glare; Low blue light mode
•	User controls Exit; Information; Management; Menu; Power control; Input control; Brightness+; Image; Color
•	Display size (diagonal) 21.5"
•	Display size (diagonal, metric) 54.6 cm (21.5")
•	Camera No integrated camera
•	Environmental
•	Operating temperature: 5 to 35°C;
•	Operating humidity: 20 to 80% non-condensing;
•	Power 100 - 240 VAC 50/60 Hz
•	Power consumption 20 W (maximum), 18.5 W (typical), 0.5 W (standby)
•	Dimensions 50.43 x 4.4 x 30.02 cm (Without stand.)
•	Weight 2.84 kg (With stand.)
•	Physical security features Security lock-ready
•	Energy efficiency compliance ENERGY STAR® certified; TCO certified; EPEAT® registered; CEL Grade 1
•	Certification and compliance
•	Australian-New Zealand MEPS; BIS; BSMI; CB; CCC; CE; CECP; CEL; cTUVus; EAC; ENERGY STAR®; E-standby; EUP Lot-5; EUP Lot-6; FCC;
•	ICES; ISO 9241-307; KC/KCC; NOM; VCCI; Vietnam MEPS; WEEE; Low blue light; EUP Lot-26; California Energy Commission (CEC); South
•	Africa Energy; WW application; UAE; Ukraine certificates; NRCS of South Africa
•	What's in the box Monitor; HDMI cable; Documentation; AC power cord
•	Warranty 3 year limited warranty including 3 year of parts and labour. Certain restrictions and exclusions apply.
•	Pixels per inch (ppi) 105 ppi
•	Panel bit depth 8 bit
•	Vertical viewing angle 178°
•	Horizontal viewing angle 178°
•	Bezel Narrow
•	Swivel No swivel
•	Tilt -5 to +20°
•	Pivot No pivot
•	Height adjustment range No height adjust
•	VESA mounting 100 mm x 100 mm
•	Hardness 3H
•	Screen treatment Anti-glare
•	Touch-enabled Not touch-enabled
•	Integrated privacy filter No
•	Flicker-free Yes
•	Low blue light modes Yes
•	Energy efficiency class E
•	Display scan frequency (horizontal) 30-80 KHz
•	Display scan frequency (vertical) 50-60 Hz
•	Pixel pitch 0.0831 mm x 0.241 mm